[Master Index] [Index for PublicToolbox/regutools]

# plsqr

## (PublicToolbox/regutools/plsqr.m in BrainStorm 2.0 (Alpha))

### Function Synopsis

    [X,rho,eta,F] = plsqr(A,L,W,b,k,reorth,sm)

### Help Text

    PLSQR "Preconditioned" version of the LSQR Lanczos bidiagonalization algorithm.

     [X,rho,eta,F] = plsqr(A,L,W,b,k,reorth,sm)

     Performs k steps of the `preconditioned' LSQR Lanczos
     bidiagonalization algorithm applied to the system
        min || (A*L_p) x - b || ,
     where L_p is the A-weighted generalized inverse of L.  Notice
     that the matrix W holding a basis for the null space of L must
     also be specified.

     The routine returns all k solutions, stored as columns of
     the matrix X.  The solution seminorm and the residual norm are
     returned in eta and rho, respectively.

     If the generalized singular values sm of (A,L) are also provided,
     then glsqr computes the filter factors associated with each step
     and stores them columnwise in the matrix F.

     Reorthogonalization is controlled by means of reorth:
        reorth = 0 : no reorthogonalization (default),
        reorth = 1 : reorthogonalization by means of MGS,
        reorth = 2 : Householder-reorthogonalization.

### Cross-Reference Information

This function calls

    app_hh                             C:\BrainStorm_2001\PublicToolbox\regutools\app_hh.m
    gen_hh                             C:\BrainStorm_2001\PublicToolbox\regutools\gen_hh.m
    lsolve                             C:\BrainStorm_2001\PublicToolbox\regutools\lsolve.m
    ltsolve                            C:\BrainStorm_2001\PublicToolbox\regutools\ltsolve.m
    pinit                              C:\BrainStorm_2001\PublicToolbox\regutools\pinit.m
    pythag                             C:\BrainStorm_2001\PublicToolbox\regutools\pythag.m

### Listing of function C:\BrainStorm_2001\PublicToolbox\regutools\plsqr.m

    function [X,rho,eta,F] = plsqr(A,L,W,b,k,reorth,sm)
    %PLSQR "Preconditioned" version of the LSQR Lanczos bidiagonalization algorithm.
    %
    % [X,rho,eta,F] = plsqr(A,L,W,b,k,reorth,sm)
    %
    % Performs k steps of the `preconditioned' LSQR Lanczos
    % bidiagonalization algorithm applied to the system
    %    min || (A*L_p) x - b || ,
    % where L_p is the A-weighted generalized inverse of L.  Notice
    % that the matrix W holding a basis for the null space of L must
    % also be specified.
    %
    % The routine returns all k solutions, stored as columns of
    % the matrix X.  The solution seminorm and the residual norm are
    % returned in eta and rho, respectively.
    %
    % If the generalized singular values sm of (A,L) are also provided,
    % then glsqr computes the filter factors associated with each step
    % and stores them columnwise in the matrix F.
    %
    % Reorthogonalization is controlled by means of reorth:
    %    reorth = 0 : no reorthogonalization (default),
    %    reorth = 1 : reorthogonalization by means of MGS,
    %    reorth = 2 : Householder-reorthogonalization.

    % References: C. C. Paige & M. A. Saunders, "LSQR: an algorithm for
    % sparse linear equations and sparse least squares", ACM Trans.
    % Math. Software 8 (1982), 43-71.
    % M. Hanke, "Regularization with differential operators.  An itera-
    % tive approach", J. Numer. Funct. Anal. Optim. 13 (1992), 523-540.

    % Per Christian Hansen, UNI-C, 05/26/93.

    % The fudge threshold is used to prevent filter factors from exploding.
    fudge_thr = 1e-4;

    % Initialization
    if (k < 1), error('Number of steps k must be positive'), end
    if (nargin==5), reorth = 0; end
    if (nargout==4 & nargin<7), error('Too few input arguments'), end
    [m,n] = size(A); X = zeros(n,k); [pp,n1] = size(L);
    if (n1 ~= n | m < n | n < pp)
      error('Incorrect dimensions of A and L')
    end
    if (reorth==0)
      UV = 0;
    elseif (reorth==1)
      U = zeros(m,k); V = zeros(pp,k); UV = 1;
    elseif (reorth==2)
      if (k>=n), error('No. of iterations must satisfy k < n'), end
      UV = 0; HHU = zeros(m,k); HHV = zeros(pp,k);
      HHalpha = zeros(1,k); HHbeta = HHalpha;
    else
      error('Illegal reorth')
    end
    if (nargout > 1)
      eta = zeros(k,1); rho = eta;
      c2 = -1; s2 = 0; xnorm = 0; z = 0;
    end
    if (nargin==7)
      [ls,ms] = size(sm);
      F = zeros(ls,k); Fv = zeros(ls,1); Fw = Fv;
      s = (sm(:,1)./sm(:,2)).^2;
    end

    % Prepare for computations with L_p.
    [NAA,x_0] = pinit(W,A,b);

    % By subtracting the component A*x_0 from b we ensure that
    % the corrent residual norms are computed.
    b = b - A*x_0;

    % Prepare for LSQR iteration.
    v = zeros(pp,1); x = v; beta = norm(b);
    if (beta==0), error('Right-hand side must be nonzero'), end
    if (reorth==2)
      [beta,HHbeta(1),HHU(:,1)] = gen_hh(b);
    end
    u = b/beta; if (UV), U(:,1) = u; end
    r = ltsolve(L,A'*u,W,NAA); alpha = norm(r);
    if (reorth==2)
      [alpha,HHalpha(1),HHV(:,1)] = gen_hh(r);
    end
    v = r/alpha; if (UV), V(:,1) = v; end
    phi_bar = beta; rho_bar = alpha; w = v;
    if (nargin==7), Fv = s/(alpha*beta); Fw = Fv; end

    % Perform Lanczos bidiagonalization with/without reorthogonalization.
    for i=2:k+1

      alpha_old = alpha; beta_old = beta;

      % Compute (A*L_p)*v - alpha*u.
      p = A*lsolve(L,v,W,NAA) - alpha*u;
      if (reorth==0)
        beta = norm(p); u = p/beta;
      elseif (reorth==1)
        for j=1:i-1, p = p - (U(:,j)'*p)*U(:,j); end
        beta = norm(p); u = p/beta;
      else
        for j=1:i-1
          p(j:m) = app_hh(p(j:m),HHbeta(j),HHU(j:m,j));
        end
        [beta,HHbeta(i),HHU(i:m,i)] = gen_hh(p(i:m));
        u = zeros(m,1); u(i) = 1;
        for j=i:-1:1
          u(j:m) = app_hh(u(j:m),HHbeta(j),HHU(j:m,j));
        end
      end

      % Compute L_p'*A'*u - beta*v.
      r = ltsolve(L,A'*u,W,NAA) - beta*v;
      if (reorth==0)
        alpha = norm(r); v = r/alpha;
      elseif (reorth==1)
        for j=1:i-1, r = r - (V(:,j)'*r)*V(:,j); end
        alpha = norm(r); v = r/alpha;
      else
        for j=1:i-1
          r(j:pp) = app_hh(r(j:pp),HHalpha(j),HHV(j:pp,j));
        end
        [alpha,HHalpha(i),HHV(i:pp,i)] = gen_hh(r(i:pp));
        v = zeros(pp,1); v(i) = 1;
        for j=i:-1:1
          v(j:pp) = app_hh(v(j:pp),HHalpha(j),HHV(j:pp,j));
        end
      end

      % Store U and V if necessary.
      if (UV), U(:,i) = u; V(:,i) = v; end

      % Construct and apply orthogonal transformation.
      rrho = pythag(rho_bar,beta); c1 = rho_bar/rrho;
      s1 = beta/rrho; theta = s1*alpha; rho_bar = -c1*alpha;
      phi = c1*phi_bar; phi_bar = s1*phi_bar;

      % Compute solution norm and residual norm if necessary;
      if (nargout > 1)
        delta = s2*rrho; gamma_bar = -c2*rrho; rhs = phi - delta*z;
        z_bar = rhs/gamma_bar; eta(i-1) = pythag(xnorm,z_bar);
        gamma = pythag(gamma_bar,theta);
        c2 = gamma_bar/gamma; s2 = theta/gamma;
        z = rhs/gamma; xnorm = pythag(xnorm,z);
        rho(i-1) = abs(phi_bar);
      end

      % If required, compute the filter factors.
      if (nargin==7)

        if (i==2)
          Fv_old = Fv;
          Fv  = Fv.*(s - beta^2 - alpha_old^2)/(alpha*beta);
          F(:,i-1) = (phi/rrho)*Fw;
        else
          tmp = Fv;
          Fv = (Fv.*(s - beta^2 - alpha_old^2) - ...
                     Fv_old*alpha_old*beta_old)/(alpha*beta);
          Fv_old = tmp;
          F(:,i-1) = F(:,i-2) + (phi/rrho)*Fw;
        end
        if (i > 3)
          f = find(abs(F(:,i-2)-1) < fudge_thr & abs(F(:,i-3)-1) < fudge_thr);
          if (length(f) > 0), F(f,i-1) = ones(length(f),1); end
        end
        Fw = Fv - (theta/rrho)*Fw;

      end

      % Update the solution.
      x = x + (phi/rrho)*w; w = v - (theta/rrho)*w;
      X(:,i-1) = lsolve(L,x,W,NAA) + x_0;

    end

Produced by color_mat2html, a customized BrainStorm 2.0 (Alpha) version of mat2html on Tue Nov 2 16:17:59 2004
Cross-Directory links are: ON