topics - functions - index - search

inv_recon.m

Multiplication of (generalized) inverse with data matrix
If dim~=1, dim rows of the inverse are considered to belong to one location in the source space
and for the solution only the absolute value for every location is output
More measurement points (electrodes, sensors) than inverse coefficients are
allowed (only the first measurement points are used), but not vice versa
Different rows of rec correpond to different locations in the source space
Different columns of rec correspond to different data points (time points)